Spring damper system for the arm

K in x, k in y

Write dynamics for arm??

Get check within theta space instead of cartesian